                                                                               NetVision Corp.
                                                                               Mar. 09, 2026


This document describes the Full package and how to install applications.

1. About Full package
 This Full package contains some sortwares and documents to use SVI-09.
 The contents of Full package are as follows:

  /Doc folder           ... Contains the documents such as software manual or hardware manual.
  /FPGA&Firm&PLL folder ... Contains the latest firmware and FPGA and PLL data.
  /UpdateAppl folder    ... Contains applications for updating FW and FPGA.
  /UVC_mode folder      ... Contains applications, driver, and documents for UVC mode.
  /Vendor_mode folder   ... Contains applications, driver, and documents for Vendor mode.
  History_en.txt        ... Describes the contents of updates.  
  Readme_en.txt         ... This file.
  Software_License_Agreement_en.pdf  ... The license agreement for softwares and materials in CD-ROM.

  * UVC mode is DSW 7-OFF, 8-OFF, and vendor mode is DSW 7-OFF, 8-ON.

2. Contents of UVC_mode folder
  /Appl_x64 folder   ... Contains applications for 64-bit UVC mode.
  /Driver_x64 folder ... Contains the device driver for 64-bit UVC mode.
  /Runtime folder    ... Runtime provided by Microsoft required to install NVCap.

3. Contents of Vendor_mode folder
  /Appl_x64 folder   ... Contains applications for 64-bit Vendor mode.
  /Driver_x64 folder ... Contains the device driver for 64-bit Vendor mode.
  /SVI-source folder ... Contains files necessary for application development.

4．How to Install Device Driver for SVI-09
 [1] Connect SVI-09 and PC via a USB3.0 cable to turn on the power of SVI-09.
 [2] The OS would request to install the device driver, then set the Full package into your Full package.
    The driver is in "Driver_x64" folder in the Full package.
    * Select "Driver_x64" when you use the OS for 64-bit

5. How to Install Application
 [1] Applications are contained in the Appl_x64 folder of
    each mode folder on the Full package, so copy all the contents to your hard disk.
    * Select one of the folders that suits your OS.

 [2] For instructions on how to use the application, refer to the manuals in Doc folder
    of each mode folder in the Full package.
    * When using multiple SVI-09 in vendor mode, create as many APP folders on the HDD
     as there are SVI-09.
      It is no problem that the contents of each folder can be the same.

6. FW, FPGA update
 [1] Necessary update tools is contains in the UpdateAppl folder of the Full package, 
    so copy it to your hard disk. Please copy and use the folder that matches the OS bit.

 [2] For details on how to update, refer to "SVMUpdater_Software_Manual" in the Full package.
    * FW and FPGA updates cannot be done in quick succession. 
      To update more than one, exit SVMupdate after updating one item, power off the SVI-09 board,
     and power on again to update next one.

7.Notes
 [1] Please use USB 3.0.
 [2] The supported OS is 10 and 11 for Windows.
 [3] When using multiple SVI-09, up to 4 boards can be used.
 [4] When using this system, do not run other applications running on the PC.
    If other applications are heavily loaded, this system may be affected. 
 [5] When you use it in vendor mode, SVI-09 is not mounted a clock generator, 
    so the PLL setting value cannot be rewritten. The initial value is set at 54MHz on the FPGA.
     After turning on the power, you can either temporarily change it
    with our application SVImon.exe or temporarily change it with the API.
     The PLL file are ones that the file name starting with the character string "s9"
    in the FPGA&Firm&PLL folder in the Full package. 
 [6] When you use multiple SVI-09 boards in vendor mode, please open SVImon.exe and SVIctl.exe
    in each APP folder.
     If you open multiple boards in the same folder, an error occurs and you cannot use.

8. Support
  For inquiries, please contact us via the contact page below..
    https://www.net-vision.co.jp/inquiry/